**Assignment-4**

|  |  |
| --- | --- |
| BATCH | B12-6A2E |
| TEAM ID | PNT2022TMID01821 |
| TEAM MEMBERS | SABARINATHAN G -7376191EC249 (TEAM LEAD)  PATHMALOSHAN C – 7376191EC224  PRANEETH R – 7376191EC231  RITHIK M – 7376191EC246 |
| PROJECT | IOT Based Safety Gadget for Child Safety Monitoring and Notification |

# ASSIGNMENT 4

Write code and connections in wokwi for ultrasonic sensor. Whenever distance is less than 100 cm send "alert" to IBM cloud and display in device recent events.

Upload document with wokwi share link and images of IBM cloud.

# CODE

#include <WiFi.h>

#include <PubSubClient.h> #include <ArduinoJson.h>

WiFiClient wifiClient; #define ORG "mz6rat"

#define DEVICE\_TYPE "arduino"

#define DEVICE\_ID "54321"

#define TOKEN "26072002"

#define speed 0.034

char server[] = ORG ".messaging.internetofthings.ibmcloud.com"; char publishTopic[] = "iot-2/evt/Data/fmt/json";

char topic[] = "iot-2/cmd/home/fmt/String"; char authMethod[] = "use-token-auth";

char token[] = TOKEN;

char clientId[] = "d:" ORG ":" DEVICE\_TYPE ":" DEVICE\_ID;

PubSubClient client(server, 1883, wifiClient); void publishData();

const int trigpin=5; const int echopin=18; String command; String data="";

long duration; int dist;

void setup()

{

**Serial**.begin(115200); pinMode(trigpin, OUTPUT);

pinMode(echopin, INPUT); wifiConnect(); mqttConnect();

}

void loop() {

publishData(); delay(500);

if (!client.loop()) { mqttConnect();

}

}

void wifiConnect() {

**Serial**.print("Connecting to "); **Serial**.print("Wifi"); WiFi.begin("Wokwi-GUEST", "", 6);

while (WiFi.status() != WL\_CONNECTED) { delay(500);

**Serial**.print(".");

}

**Serial**.print("WiFi connected, IP address: "); **Serial**.println(WiFi.localIP());

}

void mqttConnect() {

if (!client.connected()) {

**Serial**.print("Reconnecting MQTT client to "); **Serial**.println(server); while (!client.connect(clientId, authMethod, token)) {

**Serial**.print("."); delay(1000);

}

initManagedDevice();

**Serial**.println();

}

}

void initManagedDevice() {

if (client.subscribe(topic)) { **Serial**.println(client.subscribe(topic)); **Serial**.println("subscribe to cmd OK");

} else {

**Serial**.println("subscribe to cmd FAILED");

}

}

void publishData()

{

digitalWrite(trigpin,LOW); digitalWrite(trigpin,HIGH); delayMicroseconds(10); digitalWrite(trigpin,LOW);

duration=pulseIn(echopin,HIGH); dist=duration\*speed/2;

if(dist<100){ DynamicJsonDocument doc(1024); String payload; doc["AlertDistance:"]=dist; serializeJson(doc, payload); delay(3000); **Serial**.print("\n");

**Serial**.print("Sending payload: ");

**Serial**.println(payload);

if (client.publish(publishTopic, (char\*) payload.c\_str())) {

**Serial**.println("Publish OK");

} else {

**Serial**.println("Publish FAILED");

}

}

}

# WOKWI LINK:

<https://wokwi.com/projects/346571307833360979>

# OUTPUT:



